{
  "schema_version": "1.4.0",
  "id": "GHSA-f3rr-2f3x-3pqj",
  "modified": "2022-05-17T05:05:46Z",
  "published": "2022-05-17T05:05:46Z",
  "aliases": [
    "CVE-2013-4219"
  ],
  "details": "Multiple integer overflows in the Intel WiMAX Network Service through 1.5.2 for Intel Wireless WiMAX Connection 2400 devices allow remote attackers to cause a denial of service (component crash) or possibly execute arbitrary code via an L5 connection with a crafted PDU value that triggers a heap-based buffer overflow within (1) L5SocketsDispatcher.c or (2) L5Connector.c.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2013-4219"
    },
    {
      "type": "WEB",
      "url": "https://bugzilla.redhat.com/show_bug.cgi?id=911129"
    },
    {
      "type": "WEB",
      "url": "http://www.openwall.com/lists/oss-security/2013/08/08/17"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2013-08-25T03:27:00Z"
  }
}