{
  "schema_version": "1.4.0",
  "id": "GHSA-fmw2-jxvh-9jcr",
  "modified": "2022-05-17T05:34:22Z",
  "published": "2022-05-17T05:34:22Z",
  "aliases": [
    "CVE-2011-4508"
  ],
  "details": "The HMI web server in Siemens WinCC flexible 2004, 2005, 2007, and 2008 before SP3; WinCC V11 (aka TIA portal) before SP2 Update 1; the TP, OP, MP, Comfort Panels, and Mobile Panels SIMATIC HMI panels; WinCC V11 Runtime Advanced; and WinCC flexible Runtime generates predictable authentication tokens for cookies, which makes it easier for remote attackers to bypass authentication via a crafted cookie.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2011-4508"
    },
    {
      "type": "WEB",
      "url": "http://www.siemens.com/corporate-technology/pool/de/forschungsfelder/siemens_security_advisory_ssa-345442.pdf"
    },
    {
      "type": "WEB",
      "url": "http://www.us-cert.gov/control_systems/pdf/ICSA-12-030-01.pdf"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-287"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2012-02-03T20:55:00Z"
  }
}