{
  "schema_version": "1.4.0",
  "id": "GHSA-f8w3-7f86-fvgw",
  "modified": "2022-05-01T07:34:16Z",
  "published": "2022-05-01T07:34:16Z",
  "aliases": [
    "CVE-2006-6055"
  ],
  "details": "Stack-based buffer overflow in A5AGU.SYS 1.0.1.41 for the D-Link DWL-G132 wireless adapter allows remote attackers to execute arbitrary code via a 802.11 beacon request with a long Rates information element (IE).",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2006-6055"
    },
    {
      "type": "WEB",
      "url": "http://projects.info-pull.com/mokb/MOKB-13-11-2006.html"
    },
    {
      "type": "WEB",
      "url": "http://secunia.com/advisories/22860"
    },
    {
      "type": "WEB",
      "url": "http://securitytracker.com/id?1017215"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/21032"
    },
    {
      "type": "WEB",
      "url": "http://www.vupen.com/english/advisories/2006/4488"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2006-11-22T01:07:00Z"
  }
}