{
  "schema_version": "1.4.0",
  "id": "GHSA-f8cr-xgwc-mr3c",
  "modified": "2022-05-01T06:51:41Z",
  "published": "2022-05-01T06:51:41Z",
  "aliases": [
    "CVE-2006-1670"
  ],
  "details": "Control cards for Cisco Optical Networking System (ONS) 15000 series nodes before 20060405 allow remote attackers to cause a denial of service (memory exhaustion and possibly card reset) by sending an invalid response when the final ACK is expected, aka bug ID CSCei45910.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2006-1670"
    },
    {
      "type": "WEB",
      "url": "https://exchange.xforce.ibmcloud.com/vulnerabilities/25643"
    },
    {
      "type": "WEB",
      "url": "http://secunia.com/advisories/19553"
    },
    {
      "type": "WEB",
      "url": "http://securitytracker.com/id?1015872"
    },
    {
      "type": "WEB",
      "url": "http://www.cisco.com/warp/public/707/cisco-sa-20060405-ons.shtml"
    },
    {
      "type": "WEB",
      "url": "http://www.osvdb.org/24434"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/17384"
    },
    {
      "type": "WEB",
      "url": "http://www.vupen.com/english/advisories/2006/1256"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2006-04-07T10:04:00Z"
  }
}