{
  "schema_version": "1.4.0",
  "id": "GHSA-f8x5-847r-2pc6",
  "modified": "2022-05-17T03:52:03Z",
  "published": "2022-05-17T03:52:03Z",
  "aliases": [
    "CVE-2016-3988"
  ],
  "details": "Multiple stack-based buffer overflows in the NTP time-server interface on Meinberg IMS-LANTIME M3000, IMS-LANTIME M1000, IMS-LANTIME M500, LANTIME M900, LANTIME M600, LANTIME M400, LANTIME M300, LANTIME M200, LANTIME M100, SyncFire 1100, and LCES devices with firmware before 6.20.004 allow remote attackers to obtain sensitive information, modify data, or cause a denial of service via a crafted parameter in a POST request.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:L/I:L/A:L"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2016-3988"
    },
    {
      "type": "WEB",
      "url": "https://ics-cert.us-cert.gov/advisories/ICSA-16-175-03"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2016-07-03T14:59:00Z"
  }
}