{
  "schema_version": "1.4.0",
  "id": "GHSA-f995-82f4-v3q4",
  "modified": "2022-05-14T03:24:13Z",
  "published": "2022-05-14T03:24:13Z",
  "aliases": [
    "CVE-2015-9136"
  ],
  "details": "In Android before 2018-04-05 or earlier security patch level on Qualcomm Snapdragon Mobile and Snapdragon Wear MDM9206, MDM9607, MDM9640, MDM9650, SD 210/SD 212/SD 205, SD 425, SD 430, SD 450, SD 600, SD 625, SD 650/52, SD 808, SD 810, SD 820, SD 835, and SDX20, in pre-auth request, Host driver uses FT IEs sent by the supplicant. A buffer overflow may occur if FT IEs sent by the supplicant are larger than the expected value.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2015-9136"
    },
    {
      "type": "WEB",
      "url": "https://source.android.com/security/bulletin/2018-04-01"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/103671"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-04-18T14:29:00Z"
  }
}