{
  "schema_version": "1.4.0",
  "id": "GHSA-g3rx-mv5m-cpx3",
  "modified": "2022-05-24T16:45:32Z",
  "published": "2022-05-24T16:45:32Z",
  "aliases": [
    "CVE-2018-4025"
  ],
  "details": "An exploitable denial-of-service vulnerability exists in the XML_GetRawEncJpg Wi-Fi command of the NT9665X Chipset firmware, running on the Anker Roav A1 Dashcam, version RoavA1SWV1.9. A specially crafted packet can cause an invalid memory dereference, resulting in a device reboot.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-4025"
    },
    {
      "type": "WEB",
      "url": "https://talosintelligence.com/vulnerability_reports/TALOS-2018-0697"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-05-13T16:29:00Z"
  }
}