{
  "schema_version": "1.4.0",
  "id": "GHSA-fcm9-4278-c4rv",
  "modified": "2022-05-14T01:14:03Z",
  "published": "2022-05-14T01:14:03Z",
  "aliases": [
    "CVE-2018-15840"
  ],
  "details": "TP-Link TL-WR840N devices allow remote attackers to cause a denial of service (networking outage) via fragmented packets, as demonstrated by an \"nmap -f\" command.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-15840"
    },
    {
      "type": "WEB",
      "url": "https://hackingvila.wordpress.com/2019/02/17/tp-link-wireless-n-router-wr840n-buffer-overflow-cve-2018-15840"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-03-29T18:29:00Z"
  }
}