{
  "schema_version": "1.4.0",
  "id": "GHSA-fcjv-8xx2-87f8",
  "modified": "2022-05-13T01:36:44Z",
  "published": "2022-05-13T01:36:44Z",
  "aliases": [
    "CVE-2017-3193"
  ],
  "details": "Multiple D-Link devices including the DIR-850L firmware versions 1.14B07 and 2.07.B05 contain a stack-based buffer overflow vulnerability in the web administration interface HNAP service.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:A/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-3193"
    },
    {
      "type": "WEB",
      "url": "https://tools.cisco.com/security/center/viewAlert.x?alertId=52967"
    },
    {
      "type": "WEB",
      "url": "https://twitter.com/NCCGroupInfosec/status/845269159277723649"
    },
    {
      "type": "WEB",
      "url": "https://www.kb.cert.org/vuls/id/305448"
    },
    {
      "type": "WEB",
      "url": "https://www.nccgroup.trust/uk/our-research/d-link-dir-850l-web-admin-interface-vulnerable-to-stack-based-buffer-overflow/?research=Technical+advisories"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/96747"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119",
      "CWE-121"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2017-12-16T02:29:00Z"
  }
}