{
  "schema_version": "1.4.0",
  "id": "GHSA-g3gf-57p9-5vjf",
  "modified": "2022-05-13T01:18:51Z",
  "published": "2022-05-13T01:18:51Z",
  "aliases": [
    "CVE-2018-11013"
  ],
  "details": "Stack-based buffer overflow in the websRedirect function in GoAhead on D-Link DIR-816 A2 (CN) routers with firmware version 1.10B05 allows unauthenticated remote attackers to execute arbitrary code via a request with a long HTTP Host header.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-11013"
    },
    {
      "type": "WEB",
      "url": "https://0x3f97.github.io/exploit/2018/05/13/D-Link-DIR-816-A2-CN-router-stack-based-buffer-overflow"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-787"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-05-13T15:29:00Z"
  }
}