{
  "schema_version": "1.4.0",
  "id": "GHSA-ffjq-497x-2qq5",
  "modified": "2022-05-13T01:04:26Z",
  "published": "2022-05-13T01:04:26Z",
  "aliases": [
    "CVE-2017-6655"
  ],
  "details": "A vulnerability in the Fibre Channel over Ethernet (FCoE) protocol implementation in Cisco NX-OS Software could allow an unauthenticated, adjacent attacker to cause a denial of service (DoS) condition when an FCoE-related process unexpectedly reloads. This vulnerability affects Cisco NX-OS Software on the following Cisco devices when they are configured for FCoE: Multilayer Director Switches, Nexus 7000 Series Switches, Nexus 7700 Series Switches. More Information: CSCvc91729. Known Affected Releases: 8.3(0)CV(0.833). Known Fixed Releases: 8.3(0)ISH(0.62) 8.3(0)CV(0.944) 8.1(1) 8.1(0.8)S0 7.3(2)D1(0.47).",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:A/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-6655"
    },
    {
      "type": "WEB",
      "url": "https://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20170607-nxos"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/98991"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1038628"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2017-06-13T06:29:00Z"
  }
}