{
  "schema_version": "1.4.0",
  "id": "GHSA-ff2w-m4wx-849v",
  "modified": "2022-05-13T01:01:17Z",
  "published": "2022-05-13T01:01:17Z",
  "aliases": [
    "CVE-2017-2878"
  ],
  "details": "An exploitable buffer overflow vulnerability exists in the web management interface used by the Foscam C1 Indoor HD Camera running application firmware 2.52.2.43. A specially crafted HTTP request can cause a buffer overflow resulting in overwriting arbitrary data. An attacker can simply send an HTTP request to the device to trigger this vulnerability.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:H/A:N"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-2878"
    },
    {
      "type": "WEB",
      "url": "https://talosintelligence.com/vulnerability_reports/TALOS-2017-0385"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119",
      "CWE-120"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-09-19T16:29:00Z"
  }
}