{
  "schema_version": "1.4.0",
  "id": "GHSA-g66x-xcf8-6hg7",
  "modified": "2022-05-13T01:32:12Z",
  "published": "2022-05-13T01:32:12Z",
  "aliases": [
    "CVE-2018-5402"
  ],
  "details": "The Auto-Maskin DCU 210E, RP-210E, and Marine Pro Observer Android App use an embedded webserver that uses unencrypted plaintext for the transmission of the administrator PIN Impact: An attacker once authenticated can change configurations, upload new configuration files, and upload executable code via file upload for firmware updates. Requires access to the network. Affected releases are Auto-Maskin DCU-210E, RP-210E, and the Marine Pro Observer Android App. Versions prior to 3.7 on ARMv7.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-5402"
    },
    {
      "type": "WEB",
      "url": "https://www.kb.cert.org/vuls/id/176301"
    },
    {
      "type": "WEB",
      "url": "https://www.us-cert.gov/ics/advisories/icsa-20-051-04"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-10-08T15:29:00Z"
  }
}