{
  "schema_version": "1.4.0",
  "id": "GHSA-gcqr-pxrf-6rrv",
  "modified": "2022-05-17T04:19:02Z",
  "published": "2022-05-17T04:19:02Z",
  "aliases": [
    "CVE-2014-8512"
  ],
  "details": "Buffer overflow in an ActiveX control in Atx45.ocx in Schneider Electric ProClima before 6.1.7 allows remote attackers to execute arbitrary code via unspecified vectors, a different vulnerability than CVE-2014-8511.  NOTE: this may be clarified later based on details provided by researchers.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2014-8512"
    },
    {
      "type": "WEB",
      "url": "https://ics-cert.us-cert.gov/advisories/ICSA-14-350-01"
    },
    {
      "type": "WEB",
      "url": "http://download.schneider-electric.com/files?p_Doc_Ref=SEVD%202014-344-01"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2014-12-27T15:59:00Z"
  }
}