{
  "schema_version": "1.4.0",
  "id": "GHSA-g9vp-vrrf-jgjx",
  "modified": "2022-05-17T01:22:52Z",
  "published": "2022-05-17T01:22:52Z",
  "aliases": [
    "CVE-2012-3949"
  ],
  "details": "The SIP implementation in Cisco Unified Communications Manager (CUCM) 6.x and 7.x before 7.1(5b)su5, 8.x before 8.5(1)su4, and 8.6 before 8.6(2a)su1; Cisco IOS 12.2 through 12.4 and 15.0 through 15.2; and Cisco IOS XE 3.3.xSG before 3.3.1SG, 3.4.xS, and 3.5.xS allows remote attackers to cause a denial of service (service crash or device reload) via a crafted SIP message containing an SDP session description, aka Bug IDs CSCtw66721, CSCtj33003, and CSCtw84664.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2012-3949"
    },
    {
      "type": "WEB",
      "url": "http://osvdb.org/85816"
    },
    {
      "type": "WEB",
      "url": "http://secunia.com/advisories/50774"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20120926-cucm"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20120926-sip"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/55697"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2012-09-27T00:55:00Z"
  }
}