{
  "schema_version": "1.4.0",
  "id": "GHSA-gc2j-fg67-x42m",
  "modified": "2022-05-17T03:37:39Z",
  "published": "2022-05-17T03:37:39Z",
  "aliases": [
    "CVE-2016-1436"
  ],
  "details": "The General Packet Radio Switching Tunneling Protocol 1 (aka GTPv1) implementation on Cisco ASR 5000 Packet Data Network Gateway devices before 19.4 allows remote attackers to cause a denial of service (Session Manager process restart) via a crafted GTPv1 packet, aka Bug ID CSCuz46198.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2016-1436"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20160621-asr"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1036152"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2016-06-23T00:59:00Z"
  }
}