{
  "schema_version": "1.4.0",
  "id": "GHSA-h94h-73hh-m5fr",
  "modified": "2022-05-17T04:16:34Z",
  "published": "2022-05-17T04:16:34Z",
  "aliases": [
    "CVE-2015-1348"
  ],
  "details": "Heap-based buffer overflow in Aruba Instant (IAP) with firmware before 4.0.0.7 and 4.1.x before 4.1.1.2 allows remote attackers to cause a denial of service (crash or reset to factory default) via a malformed frame to the wireless interface.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2015-1348"
    },
    {
      "type": "WEB",
      "url": "http://www.arubanetworks.com/support/alerts/aruba-psa-2015-001.txt"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2015-02-03T16:59:00Z"
  }
}