{
  "schema_version": "1.4.0",
  "id": "GHSA-jcj2-x3v8-79c9",
  "modified": "2022-05-01T07:35:07Z",
  "published": "2022-05-01T07:35:07Z",
  "aliases": [
    "CVE-2006-6125"
  ],
  "details": "Heap-based buffer overflow in the wireless driver (WG311ND5.SYS) 2.3.1.10 for NetGear WG311v1 wireless adapter allows remote attackers to execute arbitrary code via an 802.11 management frame with a long SSID.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2006-6125"
    },
    {
      "type": "WEB",
      "url": "http://projects.info-pull.com/mokb/MOKB-22-11-2006.html"
    },
    {
      "type": "WEB",
      "url": "http://secunia.com/advisories/23051"
    },
    {
      "type": "WEB",
      "url": "http://securitytracker.com/id?1017275"
    },
    {
      "type": "WEB",
      "url": "http://www.kb.cert.org/vuls/id/403152"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/21251"
    },
    {
      "type": "WEB",
      "url": "http://www.vupen.com/english/advisories/2006/4674"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2006-11-27T00:07:00Z"
  }
}