{
  "schema_version": "1.4.0",
  "id": "GHSA-qjqh-pp4q-mrg7",
  "modified": "2022-08-25T00:00:28Z",
  "published": "2022-08-23T00:00:18Z",
  "aliases": [
    "CVE-2022-37133"
  ],
  "details": "D-link DIR-816 A2_v1.10CNB04.img reboots the router without authentication via /goform/doReboot. No authentication is required, and reboot is executed when the function returns at the end.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2022-37133"
    },
    {
      "type": "WEB",
      "url": "https://github.com/z1r00/IOT_Vul/blob/main/dlink/Dir816/doReboot/readme.md"
    },
    {
      "type": "WEB",
      "url": "https://www.dlink.com/en/security-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-404"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2022-08-22T15:15:00Z"
  }
}