{
  "schema_version": "1.4.0",
  "id": "GHSA-jcfg-jw2f-mp6w",
  "modified": "2022-05-13T01:48:03Z",
  "published": "2022-05-13T01:48:03Z",
  "aliases": [
    "CVE-2017-9702"
  ],
  "details": "In android for MSM, Firefox OS for MSM, QRD Android, with all Android releases from CAF using the Linux kernel, a user-space pointer is directly accessed in a camera driver.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:L/AC:L/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-9702"
    },
    {
      "type": "WEB",
      "url": "https://source.android.com/security/bulletin/pixel/2017-11-01"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2017-11-16T22:29:00Z"
  }
}