{
  "schema_version": "1.4.0",
  "id": "GHSA-jq4c-f823-cpw5",
  "modified": "2022-05-17T04:55:50Z",
  "published": "2022-05-17T04:55:50Z",
  "aliases": [
    "CVE-2013-5037"
  ],
  "details": "The HOT HOTBOX router with software 2.1.11 has a default WPS PIN of 12345670, which makes it easier for remote attackers to obtain the WPA or WPA2 pre-shared key via EAP messages.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2013-5037"
    },
    {
      "type": "WEB",
      "url": "http://packetstormsecurity.com/files/123901/HOTBOX-2.1.11-CSRF-Traversal-Denial-Of-Service.html"
    },
    {
      "type": "WEB",
      "url": "http://www.youtube.com/watch?v=CPlT09ZIj48"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "LOW",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2013-12-30T04:53:00Z"
  }
}