{
  "schema_version": "1.4.0",
  "id": "GHSA-jq9w-vj57-3rrc",
  "modified": "2024-04-04T01:22:49Z",
  "published": "2022-05-24T16:51:26Z",
  "aliases": [
    "CVE-2019-2345"
  ],
  "details": "Race condition while accessing DMA buffer in jpeg driver in Snapdragon Auto, Snapdragon Connectivity, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon Mobile, Snapdragon Wearables in MSM8909W, MSM8996AU, QCS605, SD 425, SD 427, SD 430, SD 435, SD 450, SD 625, SD 636, SD 712 / SD 710 / SD 670, SD 820, SD 820A, SD 835, SD 845 / SD 850, SDA660, SDM660, SDX20, SDX24",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:L/AC:H/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-2345"
    },
    {
      "type": "WEB",
      "url": "https://www.codeaurora.org/security-bulletin/2019/07/01/july-2019-code-aurora-security-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-362"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-07-25T17:15:00Z"
  }
}