{
  "schema_version": "1.4.0",
  "id": "GHSA-jpxh-mq89-hwp3",
  "modified": "2022-05-14T03:25:30Z",
  "published": "2022-05-14T03:25:30Z",
  "aliases": [
    "CVE-2014-9998"
  ],
  "details": "In Android before 2018-04-05 or earlier security patch level on Qualcomm Snapdragon Automobile, Snapdragon Mobile, and Snapdragon Wear IPQ4019, IPQ8064, MDM9206, MDM9607, MDM9635M, MDM9640, MDM9650, QCA4531, QCA6174A, QCA6574AU, QCA6584, QCA6584AU, QCA9377, QCA9378, QCA9379, QCA9558, QCA9880, QCA9886, QCA9980, SD 210/SD 212/SD 205, SD 425, SD 625, SD 808, SD 810, SD 820, and SDX20, while processing firmware image signature, the internal buffer may overflow if the firmware signature size is large.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2014-9998"
    },
    {
      "type": "WEB",
      "url": "https://source.android.com/security/bulletin/2018-04-01"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/103671"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-04-18T14:29:00Z"
  }
}