{
  "schema_version": "1.4.0",
  "id": "GHSA-hv57-64g7-457f",
  "modified": "2025-04-12T12:43:49Z",
  "published": "2022-05-14T03:29:27Z",
  "aliases": [
    "CVE-2014-9583"
  ],
  "details": "common.c in infosvr in ASUS WRT firmware 3.0.0.4.376_1071, 3.0.0.376.2524-g0013f52, and other versions, as used in RT-AC66U, RT-N66U, and other routers, does not properly check the MAC address for a request, which allows remote attackers to bypass authentication and execute arbitrary commands via a NET_CMD_ID_MANU_CMD packet to UDP port 9999.  NOTE: this issue was incorrectly mapped to CVE-2014-10000, but that ID is invalid due to its use as an example of the 2014 CVE ID syntax change.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2014-9583"
    },
    {
      "type": "WEB",
      "url": "https://github.com/jduck/asus-cmd"
    },
    {
      "type": "WEB",
      "url": "https://support.t-mobile.com/docs/DOC-21994"
    },
    {
      "type": "WEB",
      "url": "https://www.exploit-db.com/exploits/44524"
    },
    {
      "type": "WEB",
      "url": "http://packetstormsecurity.com/files/129815/ASUSWRT-3.0.0.4.376_1071-LAN-Backdoor-Command-Execution.html"
    },
    {
      "type": "WEB",
      "url": "http://www.exploit-db.com/exploits/35688"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2015-01-08T20:59:00Z"
  }
}