{
  "schema_version": "1.4.0",
  "id": "GHSA-hhjf-8rx4-9rp6",
  "modified": "2022-05-13T01:35:26Z",
  "published": "2022-05-13T01:35:26Z",
  "aliases": [
    "CVE-2018-0299"
  ],
  "details": "A vulnerability in the Simple Network Management Protocol (SNMP) feature of Cisco NX-OS on the Cisco Nexus 4000 Series Switch could allow an authenticated, remote attacker to cause the device to unexpectedly reload, resulting in a denial of service (DoS) condition. The vulnerability is due to incomplete validation of an SNMP poll request for a specific MIB. An attacker could exploit this vulnerability by sending a specific SNMP poll request to the targeted device. An exploit could allow the attacker to cause the device to reload, resulting in a DoS condition. Cisco Bug IDs: CSCvg10442.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:L/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-0299"
    },
    {
      "type": "WEB",
      "url": "https://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20180620-n4k-snmp-dos"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1041169"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-06-21T11:29:00Z"
  }
}