{
  "schema_version": "1.4.0",
  "id": "GHSA-hhf2-ff79-7j23",
  "modified": "2022-05-17T01:21:44Z",
  "published": "2022-05-17T01:21:44Z",
  "aliases": [
    "CVE-2016-1398"
  ],
  "details": "Buffer overflow in the web-based management interface on Cisco RV110W devices with firmware through 1.2.1.4, RV130W devices with firmware through 1.0.2.7, and RV215W devices with firmware through 1.3.0.7 allows remote authenticated users to cause a denial of service (device reload) via a crafted HTTP request, aka Bug ID CSCux86669.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:L/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2016-1398"
    },
    {
      "type": "WEB",
      "url": "https://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20160615-rv3"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1036115"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2016-07-03T21:59:00Z"
  }
}