{
  "schema_version": "1.4.0",
  "id": "GHSA-jr7j-5wrw-qxv3",
  "modified": "2022-05-13T01:35:58Z",
  "published": "2022-05-13T01:35:58Z",
  "aliases": [
    "CVE-2018-0030"
  ],
  "details": "Receipt of a specific MPLS packet may cause MPC7/8/9, PTX-FPC3 (FPC-P1, FPC-P2) line cards or PTX1K to crash and restart. By continuously sending specific MPLS packets, an attacker can repeatedly crash the line cards or PTX1K causing a sustained Denial of Service. Affected releases are Juniper Networks Junos OS with MPC7/8/9 or PTX-FPC3 (FPC-P1, FPC-P2) installed and PTX1K: 15.1F versions prior to 15.1F6-S10; 15.1 versions prior to 15.1R4-S9, 15.1R6-S6, 15.1R7; 16.1 versions prior to 16.1R3-S8, 16.1R4-S9, 16.1R5-S4, 16.1R6-S3, 16.1R7; 16.1X65 versions prior to 16.1X65-D46; 16.2 versions prior to 16.2R1-S6, 16.2R2-S5, 16.2R3; 17.1 versions prior to 17.1R1-S7, 17.1R2-S7, 17.1R3; 17.2 versions prior to 17.2R1-S4, 17.2R2-S4, 17.2R3; 17.2X75 versions prior to 17.2X75-D70, 17.2X75-D90; 17.3 versions prior to 17.3R1-S4, 17.3R2, 17.4 versions prior to 17.4R1-S2, 17.4R2. Refer to KB25385 for more information about PFE line cards.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-0030"
    },
    {
      "type": "WEB",
      "url": "https://kb.juniper.net/JSA10864"
    },
    {
      "type": "WEB",
      "url": "https://kb.juniper.net/KB25385"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1041325"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-400"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-07-11T18:29:00Z"
  }
}