{
  "schema_version": "1.4.0",
  "id": "GHSA-jrpq-3jhp-h3pc",
  "modified": "2022-05-14T03:00:55Z",
  "published": "2022-05-14T03:00:55Z",
  "aliases": [
    "CVE-2018-13989"
  ],
  "details": "Grundig Smart Inter@ctive TV 3.0 devices allow CSRF attacks via a POST request to TCP port 8085 containing a predictable ID value, as demonstrated by a /sendrcpackage?keyid=-2544&keysymbol=-4081 request to shut off the device.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:R/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-13989"
    },
    {
      "type": "WEB",
      "url": "https://packetstormsecurity.com/files/148453/Grundig-Smart-Inter-ctive-3.0-Insecure-Direct-Object-Reference.html"
    },
    {
      "type": "WEB",
      "url": "https://www.exploit-db.com/exploits/45022"
    },
    {
      "type": "WEB",
      "url": "https://www.youtube.com/watch?v=H7WYTkgtwsY"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-352"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-07-11T16:29:00Z"
  }
}