{
  "schema_version": "1.4.0",
  "id": "GHSA-jrpw-v2qc-8m5g",
  "modified": "2022-05-04T00:29:42Z",
  "published": "2022-05-04T00:29:42Z",
  "aliases": [
    "CVE-2012-0370"
  ],
  "details": "Cisco Wireless LAN Controller (WLC) devices with software 4.x, 5.x, 6.0, and 7.0 before 7.0.220.0 and 7.1 before 7.1.91.0, when WebAuth is enabled, allow remote attackers to cause a denial of service (device reload) via a sequence of (1) HTTP or (2) HTTPS packets, aka Bug ID CSCtt47435.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2012-0370"
    },
    {
      "type": "WEB",
      "url": "http://archives.neohapsis.com/archives/bugtraq/2012-02/0188.html"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20120229-wlc"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2012-03-01T01:55:00Z"
  }
}