{
  "schema_version": "1.4.0",
  "id": "GHSA-jwq5-x3fj-mjph",
  "modified": "2024-03-21T03:33:58Z",
  "published": "2022-05-24T17:39:31Z",
  "aliases": [
    "CVE-2021-3182"
  ],
  "details": "** UNSUPPORTED WHEN ASSIGNED ** D-Link DCS-5220 devices have a buffer overflow. NOTE: This vulnerability only affects products that are no longer supported by the maintainer.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:A/AC:L/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2021-3182"
    },
    {
      "type": "WEB",
      "url": "https://supportannouncement.us.dlink.com/announcement/publication.aspx?name=SAP10203"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-120",
      "CWE-787"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2021-01-19T15:15:00Z"
  }
}