{
  "schema_version": "1.4.0",
  "id": "GHSA-jx9p-pjg4-8cmj",
  "modified": "2022-05-14T03:35:06Z",
  "published": "2022-05-14T03:35:06Z",
  "aliases": [
    "CVE-2017-15323"
  ],
  "details": "Huawei DP300 V500R002C00, NIP6600 V500R001C00, V500R001C20, V500R001C30, Secospace USG6500 V500R001C00, V500R001C20, V500R001C30, TE60 V100R001C01, V100R001C10, V100R003C00, V500R002C00, V600R006C00, TP3106 V100R001C06, V100R002C00, VP9660 V200R001C02, V200R001C30, V500R002C00, V500R002C10, ViewPoint 8660 V100R008C03, ViewPoint 9030 V100R011C02, V100R011C03, eCNS210_TD V100R004C10, eSpace U1981 V200R003C30 have a DoS vulnerability caused by memory exhaustion in some Huawei products. For lacking of adequate input validation, attackers can craft and send some malformed messages to the target device to exhaust the memory of the device and cause a Denial of Service (DoS).",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:L/AC:L/PR:L/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-15323"
    },
    {
      "type": "WEB",
      "url": "http://www.huawei.com/en/psirt/security-advisories/huawei-sa-20171201-01-pse-en"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-400"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-03-09T21:29:00Z"
  }
}