{
  "schema_version": "1.4.0",
  "id": "GHSA-jxhf-r3w6-4pgq",
  "modified": "2022-05-17T03:08:44Z",
  "published": "2022-05-17T03:08:44Z",
  "aliases": [
    "CVE-2015-0772"
  ],
  "details": "Cisco TelePresence Video Communication Server (VCS) X8.5RC4 allows remote attackers to cause a denial of service (CPU consumption or device outage) via a crafted SDP parameter-negotiation request in an SDP session during a SIP connection, aka Bug ID CSCut42422.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2015-0772"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/viewAlert.x?alertId=39240"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1032540"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2015-06-12T14:59:00Z"
  }
}