{
  "schema_version": "1.4.0",
  "id": "GHSA-m8wq-c42p-jw5v",
  "modified": "2022-05-13T01:24:33Z",
  "published": "2022-05-13T01:24:33Z",
  "aliases": [
    "CVE-2015-0568"
  ],
  "details": "Use-after-free vulnerability in the msm_set_crop function in drivers/media/video/msm/msm_camera.c in the MSM-Camera driver for the Linux kernel 3.x, as used in Qualcomm Innovation Center (QuIC) Android contributions for MSM devices and other products, allows attackers to gain privileges or cause a denial of service (memory corruption) via an application that makes a crafted ioctl call.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:L/AC:L/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2015-0568"
    },
    {
      "type": "WEB",
      "url": "https://www.codeaurora.org/projects/security-advisories/multiple-issues-camera-drivers-cve-2014-9410-cve-2015-0568"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/92379"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-416"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2016-08-07T21:59:00Z"
  }
}