{
  "schema_version": "1.4.0",
  "id": "GHSA-m9pf-g7xr-pwj9",
  "modified": "2024-04-04T00:07:05Z",
  "published": "2022-05-24T16:44:38Z",
  "aliases": [
    "CVE-2018-14559"
  ],
  "details": "An issue was discovered on Tenda AC7 devices with firmware through V15.03.06.44_CN(AC7), AC9 devices with firmware through V15.03.05.19(6318)_CN(AC9), and AC10 devices with firmware through V15.03.06.23_CN(AC10). A buffer overflow vulnerability exists in the router's web server (httpd). When processing the list parameters for a post request, the value is directly written with sprintf to a local variable placed on the stack, which overrides the return address of the function, causing a buffer overflow.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2018-14559"
    },
    {
      "type": "WEB",
      "url": "https://github.com/zsjevilhex/iot/blob/master/route/tenda/tenda-02/Tenda.md"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-04-25T20:29:00Z"
  }
}