{
  "schema_version": "1.4.0",
  "id": "GHSA-mf3v-5wxm-35rf",
  "modified": "2022-05-13T01:44:42Z",
  "published": "2022-05-13T01:44:42Z",
  "aliases": [
    "CVE-2017-18330"
  ],
  "details": "Buffer overflow in AES-CCM and AES-GCM encryption via initialization vector in snapdragon automobile, snapdragon mobile and snapdragon wear in versions IPQ8074, MDM9206, MDM9607, MDM9635M, MDM9640, MDM9650, MDM9655, MSM8909W, MSM8996AU, SD 210/SD 212/SD 205, SD 410/12, SD 425, SD 427, SD 430, SD 435, SD 439 / SD 429, SD 450, SD 615/16/SD 415, SD 625, SD 632, SD 636, SD 650/52, SD 810, SD 820, SD 820A, SD 835, SDA660, SDM439, SDM630, SDM660, SDX24, Snapdragon_High_Med_2016.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:L/AC:L/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-18330"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/106128"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-01-03T15:29:00Z"
  }
}