{
  "schema_version": "1.4.0",
  "id": "GHSA-mp6x-3xwx-p53c",
  "modified": "2022-05-13T01:01:25Z",
  "published": "2022-05-13T01:01:25Z",
  "aliases": [
    "CVE-2017-2805"
  ],
  "details": "An exploitable stack-based buffer overflow vulnerability exists in the web management interface used by the Foscam C1 Indoor HD Camera. A specially crafted http request can cause a stack-based buffer overflow resulting in overwriting arbitrary data on the stack frame. An attacker can simply send an http request to the device to trigger this vulnerability.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-2805"
    },
    {
      "type": "WEB",
      "url": "https://www.talosintelligence.com/vulnerability_reports/TALOS-2017-0299"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/99190"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-787"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2017-06-21T13:29:00Z"
  }
}