{
  "schema_version": "1.4.0",
  "id": "GHSA-mp8w-5ccr-gf45",
  "modified": "2022-05-24T17:27:31Z",
  "published": "2022-05-24T17:27:31Z",
  "aliases": [
    "CVE-2020-11115"
  ],
  "details": "u'Buffer over read occurs while processing information element from beacon due to lack of check of data received from beacon' in Snapdragon Auto, Snapdragon Compute, Snapdragon Consumer Electronics Connectivity, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon Mobile, Snapdragon Voice & Music, Snapdragon Wearables in APQ8009, APQ8053, APQ8096AU, APQ8098, Bitra, Kamorta, MDM9206, MDM9207C, MDM9607, MDM9640, MDM9650, MSM8905, MSM8909W, MSM8917, MSM8920, MSM8937, MSM8940, MSM8953, MSM8996AU, MSM8998, QCA6174A, QCA6574AU, QCA9377, QCA9379, QCM2150, QCN7605, QCS405, QCS605, QM215, Rennell, SA415M, Saipan, SC8180X, SDA845, SDM429, SDM429W, SDM439, SDM450, SDM632, SDM660, SDM845, SDX20, SDX55, SM6150, SM7150, SM8150, SM8250, SXR2130",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2020-11115"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins/august-2020-bulletin"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins/august-2020-security-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2020-09-08T10:15:00Z"
  }
}