{
  "schema_version": "1.4.0",
  "id": "GHSA-mpm2-q4w3-64vg",
  "modified": "2022-05-17T03:32:07Z",
  "published": "2022-05-17T03:32:07Z",
  "aliases": [
    "CVE-2016-1327"
  ],
  "details": "Buffer overflow in the web server on Cisco DPC2203 and EPC2203 devices with firmware r1_customer_image allows remote attackers to execute arbitrary code via a crafted HTTP request, aka Bug ID CSCuv05935.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2016-1327"
    },
    {
      "type": "WEB",
      "url": "https://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20160309-cmre"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/84279"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1035235"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2016-03-09T20:59:00Z"
  }
}