{
  "schema_version": "1.4.0",
  "id": "GHSA-mph2-w5gr-qrv5",
  "modified": "2022-05-24T17:03:19Z",
  "published": "2022-05-24T17:03:19Z",
  "aliases": [
    "CVE-2019-10592"
  ],
  "details": "Possible integer overflow while multiplying two integers of 32 bit in QDCM API of get display modes as there is no check on the maximum mode count in Snapdragon Auto, Snapdragon Compute, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon Mobile, Snapdragon Voice & Music, Snapdragon Wearables in APQ8017, APQ8053, APQ8096AU, APQ8098, MDM9206, MDM9207C, MDM9607, MSM8909, MSM8909W, MSM8917, MSM8920, MSM8937, MSM8940, MSM8953, MSM8996AU, MSM8998, Nicobar, QCS405, QCS605, QM215, SDA660, SDA845, SDM429, SDM439, SDM450, SDM630, SDM632, SDM636, SDM660, SDM670, SDM710, SDM845, SDX20, SM6150, SM7150, SM8150, SM8250, SXR1130, SXR2130",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-10592"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins/november-2019-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-12-12T09:15:00Z"
  }
}