{
  "schema_version": "1.4.0",
  "id": "GHSA-q4mm-jww3-53jr",
  "modified": "2022-05-13T01:44:43Z",
  "published": "2022-05-13T01:44:43Z",
  "aliases": [
    "CVE-2017-2300"
  ],
  "details": "On Juniper Networks SRX Series Services Gateways chassis clusters running Junos OS 12.1X46 prior to 12.1X46-D65, 12.3X48 prior to 12.3X48-D40, 12.3X48 prior to 12.3X48-D60, flowd daemon on the primary node of an SRX Series chassis cluster may crash and restart when attempting to synchronize a multicast session created via crafted multicast packets.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-2300"
    },
    {
      "type": "WEB",
      "url": "https://kb.juniper.net/JSA10768"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/95400"
    },
    {
      "type": "WEB",
      "url": "http://www.securitytracker.com/id/1037597"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2017-05-30T14:29:00Z"
  }
}