{
  "schema_version": "1.4.0",
  "id": "GHSA-q4rq-hc56-f8p6",
  "modified": "2022-05-24T17:44:05Z",
  "published": "2022-05-24T17:44:05Z",
  "aliases": [
    "CVE-2020-35226"
  ],
  "details": "NETGEAR JGS516PE/GS116Ev2 v2.6.0.43 devices allow unauthenticated users to modify the switch DHCP configuration by sending the corresponding write request command.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2020-35226"
    },
    {
      "type": "WEB",
      "url": "https://research.nccgroup.com/2021/03/08/technical-advisory-multiple-vulnerabilities-in-netgear-prosafe-plus-jgs516pe-gs116ev2-switches"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-74"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2021-03-10T19:15:00Z"
  }
}