{
  "schema_version": "1.4.0",
  "id": "GHSA-q746-c23r-q3qq",
  "modified": "2022-05-13T01:01:28Z",
  "published": "2022-05-13T01:01:28Z",
  "aliases": [
    "CVE-2017-16346"
  ],
  "details": "An attacker could send an authenticated HTTP request to trigger this vulnerability in Insteon Hub running firmware version 1012. At 0x9d01c368 the value for the s_mac key is copied using strcpy to the buffer at 0xa000170c. This buffer is 25 bytes large, sending anything longer will cause a buffer overflow. The destination can also be shifted by using an sn_speaker parameter between \"0\" and \"3\".",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.0/AV:N/AC:L/PR:L/UI:N/S:C/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2017-16346"
    },
    {
      "type": "WEB",
      "url": "https://www.talosintelligence.com/vulnerability_reports/TALOS-2017-0484"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119",
      "CWE-120"
    ],
    "severity": "CRITICAL",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2018-08-02T19:29:00Z"
  }
}