{
  "schema_version": "1.4.0",
  "id": "GHSA-qfvq-m4vm-x9px",
  "modified": "2022-05-17T04:31:44Z",
  "published": "2022-05-17T04:31:44Z",
  "aliases": [
    "CVE-2013-2645"
  ],
  "details": "Multiple cross-site request forgery (CSRF) vulnerabilities on the TP-LINK WR1043N router with firmware TL-WR1043ND_V1_120405 allow remote attackers to hijack the authentication of administrators for requests that (1) enable FTP access (aka \"FTP directory traversal\") to /tmp via the shareEntire parameter to userRpm/NasFtpCfgRpm.htm, (2) change the FTP administrative password via the nas_admin_pwd parameter to userRpm/NasUserAdvRpm.htm, (3) enable FTP on the WAN interface via the internetA parameter to userRpm/NasFtpCfgRpm.htm, (4) launch the FTP service via the startFtp parameter to userRpm/NasFtpCfgRpm.htm, or (5) enable or disable bandwidth limits via the QoSCtrl parameter to userRpm/QoSCfgRpm.htm.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2013-2645"
    },
    {
      "type": "WEB",
      "url": "http://securityevaluators.com/knowledge/case_studies/routers/tp-link_wr1043n.php"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-352"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2014-10-06T01:55:00Z"
  }
}