{
  "schema_version": "1.4.0",
  "id": "GHSA-q7c6-x96r-hrg8",
  "modified": "2022-05-13T01:05:41Z",
  "published": "2022-05-13T01:05:41Z",
  "aliases": [
    "CVE-2012-5723"
  ],
  "details": "Cisco ASR 1000 devices with software before 3.8S, when BDI routing is enabled, allow remote attackers to cause a denial of service (device reload) via crafted (1) broadcast or (2) multicast ICMP packets with fragmentation, aka Bug ID CSCub55948.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2012-5723"
    },
    {
      "type": "WEB",
      "url": "http://www.cisco.com/c/en/us/td/docs/routers/asr1000/release/notes/asr1k_rn_rel_notes/asr1k_caveats_38s.html"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-20"
    ],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2014-04-24T10:55:00Z"
  }
}