{
  "schema_version": "1.4.0",
  "id": "GHSA-qfxx-p6hh-pg3p",
  "modified": "2024-04-04T02:00:16Z",
  "published": "2022-05-24T16:56:51Z",
  "aliases": [
    "CVE-2019-16889"
  ],
  "details": "Ubiquiti EdgeMAX devices before 2.0.3 allow remote attackers to cause a denial of service (disk consumption) because *.cache files in /var/run/beaker/container_file/ are created when providing a valid length payload of 249 characters or fewer to the beaker.session.id cookie in a GET header. The attacker can use a long series of unique session IDs.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:N/AC:L/PR:N/UI:N/S:U/C:N/I:N/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-16889"
    },
    {
      "type": "WEB",
      "url": "https://hackerone.com/reports/406614"
    },
    {
      "type": "WEB",
      "url": "https://community.ui.com/releases/New-EdgeRouter-firmware-2-0-3-has-been-released-2-0-3/e8badd28-a112-4269-9fb6-ffe3fc0e1643"
    },
    {
      "type": "WEB",
      "url": "https://mjlanders.com/2019/07/28/resource-consumption-dos-on-edgemax-v1-10-6"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-770"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2019-09-25T20:15:00Z"
  }
}