{
  "schema_version": "1.4.0",
  "id": "GHSA-q735-69hc-jw9q",
  "modified": "2022-05-17T04:06:49Z",
  "published": "2022-05-17T04:06:49Z",
  "aliases": [
    "CVE-2015-6454"
  ],
  "details": "Everest PeakHMI before 8.7.0.2, when the video server is used, allows remote attackers to cause a denial of service (incorrect pointer dereference and daemon crash) via a crafted packet.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2015-6454"
    },
    {
      "type": "WEB",
      "url": "https://ics-cert.us-cert.gov/advisories/ICSA-15-232-01"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "MODERATE",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2015-09-26T01:59:00Z"
  }
}