{
  "schema_version": "1.4.0",
  "id": "GHSA-rfw9-259h-m9m6",
  "modified": "2022-05-17T04:38:56Z",
  "published": "2022-05-17T04:38:56Z",
  "aliases": [
    "CVE-2014-4927"
  ],
  "details": "Buffer overflow in ACME micro_httpd, as used in D-Link DSL2750U and DSL2740U and NetGear WGR614 and MR-ADSL-DG834 routers allows remote attackers to cause a denial of service (crash) via a long string in the URI in a GET request.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2014-4927"
    },
    {
      "type": "WEB",
      "url": "http://osvdb.org/show/osvdb/109356"
    },
    {
      "type": "WEB",
      "url": "http://packetstormsecurity.com/files/127544/ACME-micro_httpd-Denial-Of-Service.html"
    },
    {
      "type": "WEB",
      "url": "http://www.exploit-db.com/exploits/34102"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/68746"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-119"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2014-07-24T14:55:00Z"
  }
}