{
  "schema_version": "1.4.0",
  "id": "GHSA-rfpx-7r27-mgh4",
  "modified": "2022-05-24T17:10:11Z",
  "published": "2022-05-24T17:10:11Z",
  "aliases": [
    "CVE-2019-10594"
  ],
  "details": "Stack overflow can occur when SDP is received with multiple payload types in the FMTP attribute of a video M line in Snapdragon Auto, Snapdragon Compute, Snapdragon Consumer IOT, Snapdragon Industrial IOT, Snapdragon IoT, Snapdragon Mobile, Snapdragon Voice & Music, Snapdragon Wearables in APQ8009, APQ8017, APQ8053, APQ8076, APQ8096, APQ8096AU, APQ8098, MDM9150, MDM9206, MDM9607, MDM9615, MDM9625, MDM9635M, MDM9640, MDM9645, MDM9650, MDM9655, MSM8905, MSM8909, MSM8909W, MSM8917, MSM8920, MSM8937, MSM8940, MSM8953, MSM8996AU, MSM8998, Nicobar, QCM2150, QCS605, QM215, Rennell, SC8180X, SDA660, SDA845, SDM429, SDM429W, SDM439, SDM450, SDM630, SDM632, SDM636, SDM660, SDM670, SDM710, SDM845, SDM850, SDX20, SDX24, SDX55, SM6150, SM7150, SM8150, SXR1130",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2019-10594"
    },
    {
      "type": "WEB",
      "url": "https://www.qualcomm.com/company/product-security/bulletins/march-2020-bulletin"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2020-03-05T09:15:00Z"
  }
}