{
  "schema_version": "1.4.0",
  "id": "GHSA-rfg2-mh29-8w8c",
  "modified": "2022-05-13T01:24:32Z",
  "published": "2022-05-13T01:24:32Z",
  "aliases": [
    "CVE-2015-0572"
  ],
  "details": "Multiple race conditions in drivers/char/adsprpc.c and drivers/char/adsprpc_compat.c in the ADSPRPC driver for the Linux kernel 3.x, as used in Qualcomm Innovation Center (QuIC) Android contributions for MSM devices and other products, allow attackers to cause a denial of service (zero-value write) or possibly have unspecified other impact via a COMPAT_FASTRPC_IOCTL_INVOKE_FD ioctl call.",
  "severity": [
    {
      "type": "CVSS_V3",
      "score": "CVSS:3.1/AV:L/AC:H/PR:L/UI:N/S:U/C:H/I:H/A:H"
    }
  ],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2015-0572"
    },
    {
      "type": "WEB",
      "url": "https://source.codeaurora.org/quic/la/kernel/msm-3.10/commit/?id=34ad3d34fbff11b8e1210b9da0dac937fb956b61"
    },
    {
      "type": "WEB",
      "url": "https://source.codeaurora.org/quic/la/kernel/msm/commit/?id=8fb32c3a8147b82e2bb159b3f70d803c9e68899b"
    },
    {
      "type": "WEB",
      "url": "https://www.codeaurora.org/race-condition-leading-arbitrary-null-write-adsp-using-ioctl-compatfastrpcioctlinvokefd-cve-2015"
    },
    {
      "type": "WEB",
      "url": "http://source.android.com/security/bulletin/2016-10-01.html"
    },
    {
      "type": "WEB",
      "url": "http://www.securityfocus.com/bid/93312"
    }
  ],
  "database_specific": {
    "cwe_ids": [
      "CWE-362"
    ],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2016-10-10T10:59:00Z"
  }
}