{
  "schema_version": "1.4.0",
  "id": "GHSA-rhx3-7q55-j2hw",
  "modified": "2022-05-17T04:50:42Z",
  "published": "2022-05-17T04:50:42Z",
  "aliases": [
    "CVE-2014-0721"
  ],
  "details": "The Cisco Unified SIP Phone 3905 with firmware before 9.4(1) allows remote attackers to obtain root access via a session on the test interface on TCP port 7870, aka Bug ID CSCuh75574.",
  "severity": [],
  "affected": [],
  "references": [
    {
      "type": "ADVISORY",
      "url": "https://nvd.nist.gov/vuln/detail/CVE-2014-0721"
    },
    {
      "type": "WEB",
      "url": "http://tools.cisco.com/security/center/content/CiscoSecurityAdvisory/cisco-sa-20140219-phone"
    }
  ],
  "database_specific": {
    "cwe_ids": [],
    "severity": "HIGH",
    "github_reviewed": false,
    "github_reviewed_at": null,
    "nvd_published_at": "2014-02-22T21:55:00Z"
  }
}